# Squaredifference — MindSpore Signal+ 使用手册 alpha 文档

# Squaredifference

逐元素计算两个输入数组对应元素的差的平方。

\[\text{output}_i = (\text{input0}_i - \text{input1}_i)^2\]

对于输入 input0 和 input1 中对应位置的每个元素，计算它们差的平方值。

输入：

  - input0 - 第一个输入数据地址。

  - input1 - 第二个输入数据地址。

  - length - 计算长度（对于复数类型，指复数的个数）。

  - core_mask - 核掩码（仅共享存储版本需要）。

输出：

  - output - 计算结果地址，其大小与输入相同。

支持平台：

  `FT78NE` `MT7004`

备注

- FT78NE 支持fp32, int8, int16, int32, fp64, cplx64, cplx128

- MT7004 支持fp16, fp32, int16, int32, cplx64

共享存储版本:

void i8_squaredifference_s(int8_t *input0, int8_t *input1, int8_t *output, int length, int core_mask)

void i16_squaredifference_s(int16_t *input0, int16_t *input1, int16_t *output, int length, int core_mask)

void i32_squaredifference_s(int32_t *input0, int32_t *input1, int32_t *output, int length, int core_mask)

void hp_squaredifference_s(half *input0, half *input1, half *output, int length, int core_mask)

void fp_squaredifference_s(float *input0, float *input1, float *output, int length, int core_mask)

void dp_squaredifference_s(double *input0, double *input1, double *output, int length, int core_mask)

void c64_squaredifference_s(float *input0, float *input1, float *output, int length, int core_mask)

void c128_squaredifference_s(double *input0, double *input1, double *output, int length, int core_mask)

C调用示例：

     1//FT78NE示例
     2#include <stdio.h>
     3#include <squaredifference.h>
     4
     5int main(int argc, char* argv[]) {
     6    float *input0 = (float *)0xA0000000;   // 第一个输入在DDR空间
     7    float *input1 = (float *)0xA1000000;   // 第二个输入在DDR空间
     8    float *output = (float *)0xB0000000;  // output
     9    int length = 1000;
    10    int core_mask = 0xff;
    11    fp_squaredifference_s(input0, input1, output, length, core_mask);
    12    return 0;
    13}

私有存储版本:

void i8_squaredifference_p(int8_t *input0, int8_t *input1, int8_t *output, int length)

void i16_squaredifference_p(int16_t *input0, int16_t *input1, int16_t *output, int length)

void i32_squaredifference_p(int32_t *input0, int32_t *input1, int32_t *output, int length)

void hp_squaredifference_p(half *input0, half *input1, half *output, int length)

void fp_squaredifference_p(float *input0, float *input1, float *output, int length)

void dp_squaredifference_p(double *input0, double *input1, double *output, int length)

void c64_squaredifference_p(float *input0, float *input1, float *output, int length)

void c128_squaredifference_p(double *input0, double *input1, double *output, int length)

C调用示例：

     1//FT78NE示例
     2#include <stdio.h>
     3#include <squaredifference.h>
     4
     5int main(int argc, char* argv[]) {
     6    float *input0 = (float *)0x10000000;   // 第一个输入在L2空间
     7    float *input1 = (float *)0x10001000;   // 第二个输入在L2空间
     8    float *output = (float *)0x10002000;   // output
     9    int length = 1000;
    10    fp_squaredifference_p(input0, input1, output, length);
    11    return 0;
    12}