# UniformReal — MindSpore Signal+ 使用手册 alpha 文档

# UniformReal

生成服从均匀分布的随机数序列，输出范围为 \([0, 1)\)。

\[output_i \sim \mathcal{U}(0, 1)\]

输入：

  - length - 输出数据长度。

  - seed - 随机数种子 1。

  - seed2 - 随机数种子 2。

  - core_mask(int, 可选) - 核掩码（仅适用于共享存储版本）。

输出：

  - output - 生成的随机数结果地址。

支持平台：

  `FT78NE` `MT7004`

备注

- FT78NE 支持 fp32

- MT7004 支持 fp32, fp16

- 随机数生成基于输入种子 seed 与 seed2，相同的种子对应确定性输出。

共享存储版本:

void fp_uniform_real_s(float *output, int length, int seed, int seed2, int core_mask)

void hp_uniform_real_s(half *output, int length, int seed, int seed2, int core_mask)

  C 调用示例：

       1// FT78NE 示例
       2#include <stdio.h>
       3
       4int main(int argc, char* argv[]) {
       5    float *output = (float *)0xA0000000;   // output 在 DDR 空间
       6    int length = 1024;
       7    int seed = 1234;
       8    int seed2 = 5678;
       9    int core_mask = 0xff;
      10    fp_uniform_real_s(output, length, seed, seed2, core_mask);
      11    return 0;
      12}

私有存储版本:

void fp_uniform_real_p(float *output, int length, int seed, int seed2)

void hp_uniform_real_p(half *output, int length, int seed, int seed2)

  C 调用示例：

       1// MT7004 示例
       2#include <stdio.h>
       3
       4int main(int argc, char* argv[]) {
       5    float *output = (float *)0x10010000;
       6    int length = 1024;
       7    int seed = 1234;
       8    int seed2 = 5678;
       9    fp_uniform_real_p(output, length, seed, seed2);
      10    return 0;
      11}