# Reshape — MindSpore Signal+ 使用手册 alpha 文档

# Reshape

对输入张量进行重塑操作。在底层实现上，由于张量形状仅由参数定义，该算子执行从输入地址到输出地址的连续数据拷贝。

\[output_i = input_i\]

输入：

  - input - 输入数据起始地址。

  - length - 需拷贝的元素个数。对于复数类型，length 表示复数的个数。

  - core_mask(int, 可选) - 核掩码（仅适用于共享存储版本）。

输出：

  - output - 输出数据起始地址。

支持平台：

  `FT78NE` `MT7004`

备注

- FT78NE 支持 int8, int16, int32, fp32, fp64, c64, c128

- MT7004 支持 fp16, fp32, int16, int32, c64

- 对于复数类型（c64 / c128），算子会自动处理实部和虚部的连续拷贝，其迁移字节数是普通类型的两倍。

共享存储版本:

void i8_reshape_s(int8_t *input, int8_t *output, int length, int core_mask)

void i16_reshape_s(int16_t *input, int16_t *output, int length, int core_mask)

void i32_reshape_s(int *input, int *output, int length, int core_mask)

void hp_reshape_s(half *input, half *output, int length, int core_mask)

void fp_reshape_s(float *input, float *output, int length, int core_mask)

void dp_reshape_s(double *input, double *output, int length, int core_mask)

void c64_reshape_s(float *input, float *output, int length, int core_mask)

void c128_reshape_s(double *input, double *output, int length, int core_mask)

  C调用示例：

       1//FT78NE示例（共享存储，多核并行拷贝）
       2#include <stdio.h>
       3#include "78NE/utils.h"
       4
       5int main(int argc, char* argv[]) {
       6    float *input = (float *)0xA0000000;   // DDR 空间
       7    float *output = (float *)0xB0000000;  // DDR 空间
       8    int length = 960001;
       9    int core_mask = 0x0B;                 // 使用逻辑核 0, 1, 2
      10    fp_reshape_s(input, output, length, core_mask);
      11    return 0;
      12}

私有存储版本:

void i8_reshape_p(int8_t *input, int8_t *output, int length)

void i16_reshape_p(int16_t *input, int16_t *output, int length)

void i32_reshape_p(int32_t *input, int32_t *output, int length)

void hp_reshape_p(half *input, half *output, int length)

void fp_reshape_p(float *input, float *output, int length)

void dp_reshape_p(double *input, double *output, int length)

void c64_reshape_p(float *input, float *output, int length)

void c128_reshape_p(double *input, double *output, int length)

  C调用示例：

       1//MT7004 示例（私有存储，单核拷贝）
       2#include <stdio.h>
       3
       4int main(int argc, char* argv[]) {
       5    float *input = (float *)0x10810000;
       6    float *output = (float *)0x10820000;
       7    int length = 1024;
       8    fp_reshape_p(input, output, length);
       9    return 0;
      10}