# RandomStandardNormal — MindSpore Signal+ 使用手册 alpha 文档

# RandomStandardNormal

生成服从标准正态分布 \(\mathcal{N}(0, 1)\) 的随机数序列。

\[output_i \sim \mathcal{N}(0, 1)\]

输入：

  - length - 输出数据长度。

  - seed - 随机数种子，用于控制生成序列的随机性。

  - core_mask(int, 可选) - 核掩码（仅适用于共享存储版本）。

输出：

  - output - 生成的标准正态分布随机数地址。

支持平台：

  `FT78NE` `MT7004`

备注

- FT78NE 支持 fp32

- MT7004 支持 fp32, fp16

- 相同的种子可生成相同的随机数序列（确定性行为）。

- 随机数生成使用 Box–Muller 算法实现。

共享存储版本:

void fp_random_standard_normal_s(float *output, int length, unsigned int seed, int core_mask)

void hp_random_standard_normal_s(half *output, int length, unsigned int seed, int core_mask)

  C 调用示例：

       1// FT78NE 示例
       2#include <stdio.h>
       3
       4int main(int argc, char* argv[]) {
       5    float *output = (float *)0xA0000000;   // output 在 DDR 空间
       6    int length = 1024;
       7    unsigned int seed = 1234;
       8    int core_mask = 0xff;
       9    fp_random_standard_normal_s(output, length, seed, core_mask);
      10    return 0;
      11}

私有存储版本:

void fp_random_standard_normal_p(float *output, int length, unsigned int seed)

void hp_random_standard_normal_p(half *output, int length, unsigned int seed)

  C 调用示例：

       1// MT7004 示例
       2#include <stdio.h>
       3
       4int main(int argc, char* argv[]) {
       5    float *output = (float *)0x10010000;
       6    int length = 1024;
       7    unsigned int seed = 1234;
       8    fp_random_standard_normal_p(output, length, seed);
       9    return 0;
      10}