# FakeQuantWithMinMaxVarsPerChannel — MindSpore Signal+ 使用手册 alpha 文档

# FakeQuantWithMinMaxVarsPerChannel

对输入数据执行按通道（Per-Channel）的逐元素伪量化运算。该算子将输入数据划分为 `channel_num` 个等长的通道，每个通道根据其对应的最小/最大值（min_val[c] / max_val[c]）独立计算缩放因子和零点，进行模拟量化与反量化。

\[channel\_size = \frac{length}{channel\_num}\]
\[\text{对于通道 } c: \quad scale_c = \frac{max\_val_c - min\_val_c}{quant\_max - quant\_min}\]
\[output_{c,i} = \text{FakeQuant}(input_{c,i}, scale_c, nudge\_min_c)\]

输入：

  - src - 输入数据地址。

  - min_val - 每个通道最小值组成的数组地址。

  - max_val - 每个通道最大值组成的数组地址。

  - length - 输入数据总长度（需能被通道数整除）。

  - quant_min - 量化后的整数最小值。

  - quant_max - 量化后的整数最大值。

  - symmetric - 是否使用对称量化。

  - channel_num - 通道数量。

  - core_mask(int, 可选) - 核掩码（仅适用于共享存储版本）。

输出：

  - output - 伪量化后的计算结果地址。

支持平台：

  `FT78NE` `MT7004`

备注

- FT78NE 支持：fp32 (fp)

- MT7004 支持：fp16 (hp), fp32 (fp)

- 输入数据的总长度 `length` 必须可以被 `channel_num` 整除。

- 每个通道的逻辑（包括 Nudge 零点调整）与单变量版本的伪量化一致。

共享存储版本:

void fp_fake_quant_with_min_max_vars_per_channel_s(float *src, float *min_val, float *max_val, float *output, int length, int quant_min, int quant_max, bool symmetric, int channel_num, int core_mask)

void hp_fake_quant_with_min_max_vars_per_channel_s(half *src, half *min_val, half *max_val, half *output, int length, int quant_min, int quant_max, bool symmetric, int channel_num, int core_mask)

  C调用示例：

       1// FT78NE 示例：fp32 类型共享存储多核计算
       2#include <stdio.h>
       3#include <stdbool.h>
       4#include "78NE/utils.h"
       5
       6int main(int argc, char* argv[]) {
       7    float *input = (float *)0xA0000000;
       8    float *min_arr = (float *)0xA1000000;
       9    float *max_arr = (float *)0xA1001000;
      10    float *output = (float *)0xB0000000;
      11    int length = 960000;
      12    int channel_num = 100;
      13    int core_mask = 0b1011;
      14
      15    fp_fake_quant_with_min_max_vars_per_channel_s(input, min_arr, max_arr, output,
      16                                                 length, 0, 255, false, channel_num, core_mask);
      17    return 0;
      18}

私有存储版本:

void fp_fake_quant_with_min_max_vars_per_channel_p(float *src, float *min_val, float *max_val, float *output, int length, int quant_min, int quant_max, bool symmetric, int channel_num)

void hp_fake_quant_with_min_max_vars_per_channel_p(half *src, half *min_val, half *max_val, half *output, int length, int quant_min, int quant_max, bool symmetric, int channel_num)

  C调用示例：

       1// MT7004 示例：fp16 (half) 类型私有存储单核计算
       2#include <stdio.h>
       3#include <stdbool.h>
       4
       5int main(int argc, char* argv[]) {
       6    half *input = (half *)0x10000000;
       7    half *min_arr = (half *)0x10008000;
       8    half *max_arr = (half *)0x10008100;
       9    half *output = (half *)0x10009000;
      10    int length = 2000;
      11    int channel_num = 10;
      12
      13    hp_fake_quant_with_min_max_vars_per_channel_p(input, min_arr, max_arr, output,
      14                                                 length, 0, 255, true, channel_num);
      15    return 0;
      16}